HEC ADC version 3.8 final release

Available at

http://wwwhep.phys.uvic.ca/ uvatlas/hec adc/hec adc.html

and in the afs directory

/afs/cern.ch/atlas/testbeam/HEC/offline/dev

Main changes from latest prerelease:

• Calibration files final, obsolete files deleted • new functionalities in the dig package : t0’s, when available, can be used.

• slow control histograms are now data card depending • hec adc version number and date of run start printed out in log file • updated manual • hv status available for each calorimeter cell for data taken in 1999 (see hec hvstat.inc):

ic hvstat(ic) =0 all ok ic hvstat(ic) =bit 1 on EST1 off/undervoltage ic hvstat(ic) =bit 2 on PAD1 off/undervoltage ic hvstat(ic) =bit 3 on PAD2 off/undervoltage ic hvstat(ic) =bit 4 on EST2 off/undervoltage

WISH correction factors in SLOW CONTROL NTUPLA?

M. Lefebvre, C.

Sbarra

Technical run monitoring software

M. Lefebvre, C. Sbarra

HEC ADC version 3.9 currently installed at the test beam, it allows

monitoring/analysing technical run data Changes since version 3.8 final release:

New geometry: only module 3 present, channel numbering unchanged, used channels tagged by ic connected(ic) =.true.

HPSS system working fine, all data collected in 2000 available from: hpsssrv1:/hpss/cern.ch/atlas/testbeam/hectestb/2000 Use rfdir, rfcp to see/get them.

M. Lefebvre, C.

Sbarra