HEC status at MPI Munich

• module assembly preparation • QC improvements • contributions to CERN repair line • electronics and cables • technical run news

stacking preparation

• stacking tables installed • HV test stands prepared • EST HV-test electrodes in workshop for modification • EST contour/dimension testing device at external firm, expect delivery in March • height control testing tool ready • copper for 5 rear modules in clean room, for 2 front modules in stock • expect start-up of stacking March 6

QC improvements

• simplified procedures • HV reduced to 2.5/2 kV • Gap capacity measurement dropped • EST dimension test and gap height control added • QC forms revised

QC forms

QC forms

CERN repair line support

• stacking table ready • 3 stacking posts at workshop • first-plate feet at workshop • hydraulics and driving rolls ready • shipment to CERN in March • Capacity measuring device and HV equipment are at CERN

electronics and cabling

• PSB production well advanced • 100 % of chips produced • 139 PSB’s produced • 130 PSB’s passed acceptance tests • production of remaining 235 PSB’s starts this week • problems with the testing set-up calibration control module unstable

• cable harnesses for one whole endcap are produced

technical run

Motivation:

• test mechanical cold test equipment • investigate noise • understand calibration pulse and signal distortion

Status:

• mechanical installation (1 front module) completed • electronics chain and daq is running • noise investigation started • shape distortion measurements under- way Problem : → figure