Pierre-Yves Duval CPPM

4 of 4

DAQ electr onic setup

HPUX

VIC8251

VIC8250

CAMAC

RIO2

MiniRODs

FEBFEBFEBFEBcarte CALIB

RAID

CORBO CBD 8210SPACSPACTDC

SCALER

TRIGG

TTC to another RIO/miniROD crate

to TRIGG

Pierre-Yves Duval CPPM

3 of 4

trigger logic modifications

LEVEL1

IT VME

TRIG B USY

SOB EOB

SOB BUSY

EOB BUSY

CLEAR B USY(commande soft)

RAID

CORBO

CORBO_EN ABLE trigger system

burst burst

SOB EOB

Reading of a limited number of event by burst, stop on last event.

inburst outburst reading outburst idle Reading of events untill EOB signal, no trigger protection. In grey, no trigger protected area NOW trigger signals are masked at EOB untill the DAQ validate them at the next SOB where it is ready to take data.

Pierre-Yves Duval CPPM

2 of 4

DAQ and trigger o verview

FEB TTC

miniROD

Phase r eading (inter -burst)

trigger

LEVEL 1

CORBO

RAID^{TDC, ADC,}

SCALER BEAM

RIO

crate VME RAID

crate VME RIO 1

VIC8251 recordings de vice can span o ver cycle SPS

CORBO_EN ABLE

Pierre-Yves Duval CPPM

1 of 4

DAQ and trigger o verview

FEB TTC

miniROD

Phase in b urst

trigger

LEVEL 1

CORBO_EN ABLE

CORBO

RAID^{TDC, ADC,}

SCALER BEAM

RIO

crate VME RAID

crate VME RIO 1