ALMY Sensors

Calibration Procedure

ffl position resolution ffl refraction angle ffl displacement measurement ffl reflection corrections

Position Resolution

ffl better than 2 μm

Refraction Angle

ffl 6-parameter function fit applied for ϑx and ϑy

Refraction Angle

ffl refraction angle determined with precision of 2-3 ¯rad

Difference in refraction for two sensor orientations

Freiburg, July 07, 2000 5

ALMY: Freiburg, July 07, 2000 6

Reflection Corrections

ffl implemented into the read-out software, applied online

The New Glass Substrate

Scan of a 10 cm diameter glass wafer:

The New Glass Substrate

Scan of a 10 cm diameter glass wafer:

ffl no calibration needed anymore !

Influence of the Light on Sensor Performance

Influence of the Light on Sensor Performance