MDT Chamber Assembly

Positioning of tube layers with accuracy ±5 μm, monitored with a laser system (see Poster):

Optical monitoring of chamber deformations:

H. Kroha, MPI für Physik, Munich Elba, 22.5.2000