Prototype Test Beam Results

• Operation of the prototype chamber with

Ar:CO_2 (93:7) gas mixture at 3 bar.

Gas chosen to avoid drift tube aging up to ≥ 0.6 C/cm.

• Determination of

r-t-relation and drift tube resolution

using the silicon strip detector beam telescope for precise track pos. meas. (σ = 11 μm):

=⇒Average drift tube position resolution as expected: 70 μm (rms)

(80 μm for Ar:N_2 :CH_4 (91:4:5) at 3 bar in 1998)

H. Kroha, MPI für Physik, Munich Elba, 22.5.2000