30 mm tubes - first hits, 790 ns deadtime

rate (kHz per tube)

3σ tube efficiency (%)

30 mm tubes - first hits, 200 ns deadtime 30 mm tubes - first and second hits, 200 ns deadtime 15 mm tubes - first hits, 200 ns deadtime 0 10 20 30 40 50 60 70 80 90

0 100 200 300 400 500