%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-10mm
\evensidemargin=-10mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
%\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{fancyplain}
 \headrulewidth 2pt
 \footrulewidth 2pt
 \plainheadrulewidth 2pt
 \plainfootrulewidth 2pt
\markboth{\sc FIGURES}{\sc FIGURES}
\markright{\sc FIGURES}
\rhead[\fancyplain{}{\bf\small\rightmark}]{\fancyplain{}{}}
%\rhead[\fancyplain{}{}]{\fancyplain{}{\small\rightmark}}
%\chead[\fancyplain{}{\small\leftmark}]{\fancyplain{}{\small\rightmark}}
\lhead[\fancyplain{}{\small\leftmark}]{\fancyplain{}{}}
%\lhead[\fancyplain{}{}]{\fancyplain{}{\bf\small\rightmark}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\rm\bf\thepage\hspace*{0.7cm}}%
{\rm\bf\thepage\hspace{0.7cm}}}
\cfoot{}
\lfoot[\fancyplain{\hspace*{0.7cm}\rm\bf\thepage}%
{\hspace*{0.7cm}\rm\bf\thepage}]%
{\fancyplain{}{}}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

\setcounter{page}{79}
%------------------------------------------       
\begin{figure}

\begin{center}
\mbox{\epsfig{figure=/.at/mdt_data/kroha/qaqc/leak_detector4.eps,height=10cm}}
\end{center}

{\bf Figure~9:} Drift tube gas leak test stand with fixtures at the endplugs as well as sliding
along the tube which allow to measure helium leakage through endplugs or tube walls into 
evacuated volumes with a mass spectrometer (system developed for endcap chambers with
many different tube lengths; Michigan).

\begin{center}
%\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/comb.eps,width=\textwidth}}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/comb_1.eps,width=\textwidth}}
\end{center}

{\bf Figure~10:} Control of tube placement on the end combs during chamber assembly
with a laser system (Rome).
\end{figure}

\clearpage

 
\begin{figure}

\begin{center}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/control.eps,width=\textwidth}}
\end{center}

{\bf Figure~11:} Schematical layout of the chamber assembly control software (MPI Munich).

\begin{center}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/control_display_color.eps,angle=-90,width=\textwidth}}
\end{center}

{\bf Figure~12:} Graphical user interface for a chamber assembly control program with display
of monitoring data (Thessaloniki).

\end{figure}
\clearpage

 
\begin{figure}

\begin{center}
%\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/diff_manometer.eps,height=12.0cm}}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/differential_1.eps,height=12.0cm}}
\end{center}

{\bf Figure~13:} Gas leak test stand for complete MDT chambers with differential manometer
and reference volume (Dubna).

\begin{center}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/dubna_leak.eps,height=10.0cm}}
\end{center}

{\bf Figure~14:} Differential manometer with reference volume for chamber leak test stands (Dubna).
\end{figure}
\clearpage
 
\begin{figure}

\begin{center}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/teststand_lmu.ps,angle=180,width=0.95\textwidth}}
\end{center}

{\bf Figure~15:} Cosmic ray test stand for the operation test of chambers at the
production sites. Several chambers can be tested simultaneously. With a tower
of three chambers, wire positions can be reconstructed (LMU Munich).
\end{figure}
\clearpage

 
\begin{figure}

\begin{center}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/qaqc/xtomo.eps,angle=90,width=0.9\textwidth}}
\end{center}

{\bf Figure~16:} X-ray tomograph setup at CERN.
\end{figure}
\clearpage

 
\begin{figure}

\begin{center}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/atlas/bos_scan_ro_v.eps,width=\textwidth}}
\end{center}

{\bf Figure~17:} 
Distributions of the residuals in $y$ and $z$ of the wire locations measured in a typical
X-ray tomograph scan of the BOS prototype chamber (readout side) with respect to an ideal wire grid.

\end{figure}
\clearpage

\end{document}
