%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%

\begin{sidewaysfigure}
%\begin{table}[p]
\renewcommand{\arraystretch}{0.95}

\begin{center}
\noindent
{\bf Table~1:} Quality control tests of drift tube materials at the chamber production sites 
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline   
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction if failed} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline

& & & &\\
\multicolumn{5}{l}{\bf Aluminum tube} \\ [1mm]

Visual inspection      & no obvious defects or holes, proper cleaning, & reject tube,    & central & 1: sample test/box \\
of inside and outside  & deburring, straightness, bar code, packing & notify supplier &         & 2: every tube before wiring \\
& & & &\\

Outer diameter envelope,   & $29970\pm 15~\mu$m & reject box & central & sample test/box \\
from 8 points on circumference   &               &  & &\\
& & & &\\

Wall thickness,   & $400\pm 30~\mu$m & reject box & central & sample test/box \\
at 8 points on circumference   &               &  & &\\
& & & &\\

Length $L$     & $L\pm 0.5$~mm ($L\le 4$~m) & reject box & central & sample test/box \\
               & $L\pm 0.7$~mm ($L >  4$~m) & & &\\
& & & &\\

Straightness   & insertion in jig  & reject tube, & central & sample test/box \\
               & without difficulties & notify supplier & & \\
\hline

& & & &\\
\multicolumn{5}{l}{\bf Wire} \\ [1mm]

Visual inspection & no defects of gold-plating,      & reject spool & central & 1: first meters and every 400~m \\
                  & proper cleaning, no kinks        &              &         & \hphantom{1:} per spool under microscope, \\
                  &                                  &              &         & 2: inspection during wiring \\
& & & &\\
\hline

& & & &\\
\multicolumn{5}{l}{\bf Endplug} \\ [1mm]

Visual inspection & proper cleaning and no obvious defects  & reject endplug, & central & 1: sample test/batch \\
                  & of plastic, O-rings, wire locator,      & notify supplier &         & 2: each endplug before wiring \\
                  & Al reference surface, crimp tube        & & &\\
& & & &\\

Outer diameter envelope,         & $30020\pm 10~\mu$m & reject batch & central & sample test/batch \\
from 8 points on circumference   &                    &              &         &            \\
({\bf optional}) & & & &\\                                                                                                                 
& & & &\\

Wire locator outer diamter       & within tolerance   & reject batch & central & sample test/batch \\
& & & &\\
\hline\hline

\end{tabular}
\end{center}

%\end{tabular}
\end{sidewaysfigure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
