%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{sidewaysfigure}
%\begin{table}[p]
\renewcommand{\arraystretch}{1.05}

\begin{center}
\noindent
{\bf Table~10:} Quality control tests of selected chambers from each production site after transport to CERN and during storage
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction on failure} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline
& & & &\\

Wire location   & $\pm 20~\mu$m rms in $y$ and $z$ & store wire location & central & 1: sample test/production site \\
measurement with& with respect to the    & data and chamber ID,          &         & 2: for chambers with expected  \\
X-ray tomograph & expected wire grid     & adjust assembly tooling&         & \hphantom{2:} mechanical problems \\
(incl.\ location&                        & in case of deviations, &         &                         \\
of wire on the  &                        & measure chambers since &         &                         \\
alignm.\ platforms) &                    & problem first detected &         &                         \\

& & & &\\
Wire tension      & within $\pm 5\%$      & store data,               & central & for one chamber/production site  \\
(osc.\ frequency) & of the nominal value  & notify production sites,  &         & at regular intervals over storage time \\
                  & at given temperature  & measure other chambers    &         & (temperature meas.\ to $\pm 1^\circ$C) \\
& & & &\\

Tube ground       & less than 100~m$\Omega$  & store data,               & central & for one chamber/production site  \\
contact resistance &                         & notify production sites,  &         & at regular intervals over        \\
                  &                          & measure other chambers    &         & storage time                     \\
& & & &\\

\hline\hline

\end{tabular}
\end{center}
\hfill

%\end{table}
\end{sidewaysfigure}
\clearpage

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
