%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{sidewaysfigure}
\renewcommand{\arraystretch}{1.10}

\begin{center}
\noindent
{\bf Table~2:} Quality control tests of drift tubes at the chamber production sites
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction if failed} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline

& & & &\\
\multicolumn{5}{l}{\bf Drift tube} \\ [1mm]

Visual inspection     & no obvious damage of tube or endplug,     & reject tube,            & local & each tube after wiring,\\
                      & no visible defects of tube and            & adjust wiring station   &       & before chamber assembly \\
                      & wire crimp, tube correctly sealed & & &\\
& & & &\\

Aluminum tube outer & less than 30.020~mm  & adjust wiring setup & local & sample test/day  \\
diameter envelope  & & & & after wiring  \\
in endplug region & & & &\\
& & & &\\

Length $L$     & $L\pm 0.5$~mm         & reject drift tube,    & local & 1: sample test/day \\
               & at $20\pm 1^\circ$C  & adjust wiring station &       & 2: each tube on chamber assembly jig \\
& & & &\\

Relative azimutal        & $\pm 10$~mrad  & reject drift tube,    & local & 1: sample test/day \\
orientation of endplugs  &                & adjust wiring station &       & 2: each tube on chamber assembly jig \\
& & & &\\

Straightness    & insertion in jig       & reject drift tube & local & 1: sample test/day  \\
                & without difficulties   &                   &       & 2: each drift tube during chamber assembly \\
& & & &\\

Ground contact  & less than 100~m$\Omega$ & repeat laser welding & local & 1: sample test/day  \\
resistance      &                         &                      &       & 2: monitoring of selected tubes over time \\
& & & &\\
\hline\hline

\end{tabular}
\end{center}

\end{sidewaysfigure}
\clearpage

%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
