%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\renewcommand{\arraystretch}{1.05}
\begin{sidewaysfigure}

\begin{center}
\noindent
{\bf Table~4:} Drift tube test equipment at the production sites
\vspace{2mm}

%\begin{footnotesize}

\begin{tabular}{|l|l|l|l|l|l|} \hline\hline
{\bf Site} & {\bf Wire tension}      & {\bf Wire position} & {\bf Leak rate}    & {\bf HV test}           & {\bf HV test}  \\
           & {\bf (osz.\ frequency)} &                     & {\bf (whole tube)} & {\bf (leakage current)} & {\bf (cosmic rate)} \\ \hline

{\bf Freiburg} & Excitation in B-field & Brandeis X-ray & Leak detector with      & HV system with & Yes \\
               &                       & system         & single-tube containers  & pA-meter       &     \\
\hline

{\bf LMU/MPI}   & CAEN SY502 meter,      & Brandeis X-ray  & Pressure rise in evacuated       & HV system with   & BNL preamp., \\
(accept.\ test) & excitation in B-field  & system, MPI jig & volume at endplug (8 tubes sim.) & 1~nA sensitivity & shaper       \\
\hline

{\bf NTU Athens} & CAEN SY502 meter,     & Brandeis X-ray  & As Pavia                      & As Pavia      & \\
                 & excitation in B-field & system          &                               &               & \\
\hline

{\bf Univ.\ Athens} & \multicolumn{5}{c|}{as NTU Athens} \\
 & \multicolumn{5}{c|}{        (after module~0)} \\ \hline

{\bf Thessaloniki} & excitation in B-field & & & CAEN SY127 (40 channels), & \\
(accept.\ test) & & & & 1~nA sensitivity HV system & \\ \hline

{\bf Frascati} & Electrostatic excit.,      & Electromagnetic, & Helium leak detector,      & CAEN SY546 (96 channel)     & Yes \\
               & multi-channel system,      & as Pavia/Rome    & 60 single-tube containers  & 1~nA sensitivity HV system, &  \\
               & integration with leak test &                  &                            & integration with leak test  &  \\
\hline

{\bf Cosenza}  & CAEN SY502 meter,          & Electromagnetic, & As Pavia,                  & CAEN SY546 (96 channel)      & \\
               & excitation in B-field      & as Pavia/Rome    & automatic control system   & 1~nA sensitivity HV system,  & \\
               & integration with leak test &                  &                            & integration with leak test   &  \\
\hline

{\bf Pavia}    & As Rome                    & Electromagnetic  & Argon mass spectrometer,   & HV system (10 channels)      &  \\
               &                            & (EMMI)           & 10 single-tube containers  & with pA-meter,               &  \\
               &                            &                  & (commercial system)        & integration with leak test   &  \\
\hline

{\bf Rome}     & Excitation in B-field,     & Electromagnetic  & As Frascati or Pavia,      & As Pavia & \\
               & multi-channel              & (EMMI)           &                            &          &  \\
\hline

{\bf NIKHEF}   & Mechanical excitation,     & Electromagnetic, & Helium leak detector,       & Multi-channel HV system,   & Yes \\
               & piezo-electric measurement & as Pavia/Rome    & multi-tube container        & integration with leak test &     \\
\hline

{\bf Dubna}    & Excitation in B-field, & Brandeis X-ray   & Helium mass spectrometer,       & CAEN SY546 (96 channel) & BNL preamp., \\
(also for MPI) & meter custom design    & system, MPI jig  & multi/single-tube containers    & 1~nA sensitivity HV system & shaper  \\
\hline

{\bf Protvino} & Excitation in B-field, & Brandeis X-ray   & Mass spectrometer &  &  \\
               & meter custom design    & system           &                   &  &  \\
\hline

{\bf Boston}   & Excitation in B-field, & Brandeis X-ray   & Mass spectrometer,   & Multi-channel HV system,   & Yes \\
               & meter custom design    & system           & multi-tube container & integration with leak test &     \\
\hline

{\bf Michigan} & As Seattle             & Electromagnetic, & Helium leak tester,         & Multi-channel HV system  &   \\
               &                        & as Pavia/Rome    & evacuated volume at end-    &  & \\
               &                        &                  & plug and moving along tube  &  & \\
\hline

{\bf Seattle}  & Excitation in B-field, & Electromagnetic, & As Michigan  & As Michigan  &  \\
               & meter custom design    & as Pavia/Rome    &              &  &   \\
\hline\hline
\end{tabular}
\end{center}

%\end{footnotesize}

\end{sidewaysfigure}
%
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
