%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{sidewaysfigure}
%\begin{table}[p]
\renewcommand{\arraystretch}{0.95}

\begin{center}
\noindent
{\bf Table~6:} Quality control tests during chamber assembly (cont.)
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction if failed} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline

& & & &\\
\multicolumn{5}{l}{\bf Assembly of tube layers} \\ [1mm]

Vacuum suction  & at nominal value & adjust & local & tube positioning on combs during glueing  \\
underpressure   & & & &\\
& & & &\\

Horizontal gaps between tubes  & not more than two adjacent     & relocate drift tubes & local & before glueing \\
                               & tube walls touching,           & & &\\
                               & no adjacent endplugs touching  & & &\\
& & & &\\

Height of endplug              & within $\pm 10~\mu$m           & relocate drift tubes & local & before glueing \\
reference surfaces             & of nominal value in $y$        & & &\\
& & & &\\

Stability of in-plane          & within $\pm 10~\mu$m            & adjust               & central & after each glueing step \\
monitor readings               & of nominal value in $y$ and $z$ &                      &         & (definition of zero of in-plane monitors), \\
(image displacement) & & & & after correction for middle \\

Sphere locations               & within $\pm 10~\mu$m            & adjust               & local   & before each glueing step, \\
                               & of nominal value in $y$ and $z$ &                      &         & with sphere and in-plane monitors \\
& & & &\\

Outer cross plate sags         & zero within $\pm 10~\mu$m       & adjust               & local & before glueing of a layer, \\
on the assembly table          & & & & measured with temporary        \\
({\bf optional})               & & & & cross plate sag monitors \\
& & & &\\

Middle cross plate sag         & zero within $\pm 20~\mu$m       & adjust               & local & before glueing of a layer, \\
on the assembly table          & & & & measured with in-plane monitors plus \\
({\bf optional})               & & & & outer cross plate sag correction \\
& & & &\\
\hline

& & & &\\
\multicolumn{5}{l}{\bf Alignment Platforms} \\ [1mm]

Angular alignment of    & within $\pm 60~\mu$rad, $\pm 200~\mu$rad,   & store data  & central & after each glueing step (initially);   \\
axial/praxial platforms & $\pm 80~\mu$rad around $x$-, $y$-, $z$-axes &             &         & tolerances incl.\ errors in rec.        \\
                        & with chamber coord.\ axes, orthog.          &             &         & of thermal and gravitational            \\
                        & $\pm 100~\mu{\mathrm rad}\times$~cross plate length&      &         & deformations with in-plane system      \\
& & & &\\

Angular alignment of    & within $\pm 200~\mu$rad, $\pm 80~\mu$rad,   & store data  & central & tolerances incl.\ errors in rec.       \\
projective platforms    & $\pm 80~\mu$rad around $x$-, $y$-, $z$-axes &             &         & of thermal and gravitational              \\
                        & with chamber coordinate axes                &             &         & deformations with in-plane system      \\
& & & &\\
\hline\hline

\end{tabular}
\end{center}

%\end{table}
\end{sidewaysfigure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
