%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{sidewaysfigure}
%\begin{table}[p]
\renewcommand{\arraystretch}{0.95}

\begin{center}
\noindent
{\bf Table~9:} Quality control tests of all assembled chambers after transport to CERN and during storage
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction on failure} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline

& & & &\\
Visual     & no visible damage  & perform possible      &   & acceptance test after transport  \\
inspection &                    & repairs, mark chamber &   & to CERN  \\                                                                     
           &                    & for X-ray tomograph   &   &          \\
           &                    & and full leak test    &   &          \\
& & & &\\

Gas leak rate & less than $2\times 10^{-8}$~bar~l/s per tube & repair gas manifold, & central & 1: full leak test for one chamber per \\
at 3 bar      &                                              & repair/disconnect    &         & transport to CERN (acceptance test)  \\
              &                                              & faulty tubes, store ID &       & or if visible damage of chamber \\
              &                                              &                        &       & 2: monitoring of pressure (at known \\
              &                                              &                        &       & temperature) over storage time \\
& & & &\\

HV stability:   & less than 5~nA/channel & replace electronics  & central & after mounting of final electronics, \\
leakage current &                        & boards; identify,    &         & with baseline gas at 3 bar and            \\
                &                        & disconnect faulty    &         & nominal and $2\times$ nominal  \\
                &                        & tubes, store ID      &         & gas gain     \\
& & & &\\
Operating test  & evaluation of performance: & replace electronics, & local   & after mounting of final electronics, \\
                & pulser test (correct       & make chamber         &         & with baseline gas at 3 bar           \\
                & connections), signals      & operational          &         & and nominal operating conditions     \\
                & from all channels, noise   &                      &         &                                      \\
                & level, random rate, uniformity &                  &         &                                      \\
& & & &\\

\hline\hline

\end{tabular}
\end{center}
\hfill

%\end{table}
\end{sidewaysfigure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
