Laser Welding of Drift Tubes

Reliable ground contact to the aluminum tube

via the aluminum ring of the endplug:

=⇒ Contact resistance < 1 mΩ, unchanged after accelerated salt spray corrosion test

H. Kroha, MPI für Physik, Munich IEEE NSS Symposium, 19/10/2000