• Measurement of wire location in tubes in the same jig as for chamber assembly.

• Resolution: 2μm.

X-Ray Wire Position Measurement

H. Kroha, MPI für Physik, Munich IEEE NSS Symposium, 19/10/2000