Assembly Jigging Precision

All components fabricated in industry, measured at MPI

Combs for tube positioning:

Tube z position: ± 4 μm (rms) Tube y position: ± 3 μm (rms) z-pitch (20^∘C): 30036 ± 0.5 μm (rms)

Sphere towers tube layer positioning:

Layer z position: ±3 μm (abs.) Layer y position: ±5 μm (abs.) y-pitch: 26039 ± 0.5 μm (rms) Spacer height: 346942±5 μm (rms)

H. Kroha, MPI für Physik, Munich IEEE NSS Symposium, 19/10/2000