Prototype Test Beam Results

• Single-tube space–drift time relation can be used over the whole beam area (1 × 1 m^2).

Allow only max. drift time to vary within 6 ns (rms) (due to varying operating conditions of drift tubes).

• Require track residual distributions as function of drift distance to be symmetric left and right of the wires

⇒ Measure wire displacements ⊥ beam with accuracy of 10 μm (rms) with respect to a reference wire.

Good correlation with wire positions from X-ray scan of the chamber:

H. Kroha, MPI für Physik, Munich IEEE NSS Symposium, 19/10/2000