Chamber Test Program

1. Required chamber leak rate at 3 bar < 2 × #tubes × tube leak rate limit is challenging but feasible.

2. HV stability test of complete chamber under varying humidity conditions.

3. Operation test of each chamber in cosmic ray tower of at least 3 chambers.

H. Kroha, MPI für Physik, Munich 18 IEEE NSS Symposium, 7 November, 2001