Preliminary Testbeam Results

• Nominal operating parameters:

Ar:CO_2(93:7) at 3 bar, gas gain 2 · 10^4 at 3080 V.

• Space-drift time relationship from calibration with silicon strip detector telescope (1999 data) with autocalibration corrections (2001 data).

• Drift tube resolution as a fct. of drift distance determined from track fit through 5 out of 6 layers.

H. Kroha, MPI für Physik, Munich 20 IEEE NSS Symposium, 7 November, 2001