% --------------------------------------------------------------------
% Aachen 99 Vortrag
% Author: H. Kroha
% --------------------------------------------------------------------
%FORMAT latex % use LATEXE format
\documentstyle[epsfig,rotating,colordvi,fancyheadings]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -17mm
\evensidemargin -17mm
\topmargin -20mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 255mm
\textwidth 190mm

\font\tenrm=cmr10

%\psdraft
\setcounter{page}{21}

\begin{document}

\pagestyle{fancyplain}
 \headrulewidth 0pt
 \plainheadrulewidth 0pt
 \footrulewidth 1pt
 \plainfootrulewidth 1pt
\rhead[\fancyplain{}{}]{\fancyplain{}{}}
\lhead[\fancyplain{}{}]{\fancyplain{}{}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\tiny IEEE NSS Symposium, 7 November, 2001}%
{\tiny IEEE NSS Symposium, 7 November, 2001}}
\cfoot{\tiny\thepage}
\lfoot[\fancyplain{}{}]%
{\fancyplain{\tiny H.~Kroha, MPI f\"ur Physik, Munich}%
{\tiny H.~Kroha, MPI f\"ur Physik, Munich}}

\fboxrule=0.8mm
\fboxsep=3mm
\parindent=0.0em
\arrayrulewidth=0.8mm
\tabcolsep=2mm
\renewcommand{\arraystretch}{1.15}
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page14
%
\begin{figure}

\begin{center}
\Blue{\fbox{\Large\bf Conclusions}}
\end{center}
\vspace{5mm}

{\bf
\begin{itemize}
\addtolength{\itemindent}{-3mm}

\item The large-scale production of the precision drift tube chambers for the
ATLAS muon spectrometer has started.

\textRed
\item The required wire positioning accuracy of {\boldmath $20~\mu$}m (rms) has been
achieved and exceeded in serial production.

\item {\boldmath $18\%$} of the 400000 drift tubes and {\boldmath $11\%$} of the 1200
MDT chambers for ATLAS have been assembled.

\item Munich/Dubna ranges above average 
with {\boldmath $35\%$} of the drift tubes and {\boldmath $17\%$} of the BOS MDT chambers
completed. Still increase of the production rate.
\textBlack

\item The performance of drift tubes and chambers meets the requirements.

\item Great care to avoid contamination of the drift tubes during assembly, test
and operation as precaution against aging.

\item Test of readout and data aquisition at high background rates 
(up to 100~Hz/cm{\boldmath ${}^2)$} in progress.

\end{itemize}
}

\end{figure}

\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
