ZEBRA bank documentation from proto97.rz banks below:

RUNH EVTH

printed by DZEDIT - DZDOC at

August 1, 1997

RUNH Run header bank

---------------------------------------------- entered file at 1-Aug-97 14:23
Bank IDH RUNH Run header bank
Author Andrei Kiryunin
ND 35
Next None
Up None
Origin None
IO-Charac 2I 3F / 2F 1I
             ---------- Description of the data words ----------
1 NRUN Run number (it is always zero!)
2 IPART Particle GEANT code
3 EBEAM Beam energy [GeV]
4 XCRY X position of the cryostat [cm]
5 YTAB Y position of the movable table [cm]
                    Information about MWPCs:
--REP level=1 (loop over chambers: 1 - 5)
  --REP level=2 (loop over planes: X and Y)
        1 Z Z position of the plane [cm]
        2 STEP Step between wires [cm]
        3 NWIRES Number of wires
  --REP level=2 -- End --
--REP level=1 -- End --

EVTH

NONE

?_{Event header bank} ND=8

EVTH

ADC channel bank

ND=3+3*NCHITS CALO �HHCALO

ADC channel bank

ND=3+3*NCHITS CALO

-

1

?

MWPC bank

ND=10+NMHITS MWPC

2

?

EVTH Event header bank

---------------------------------------------- entered file at 1-Aug-97 13:40
Bank IDH EVTH Event header bank
Author Andrei Kiryunin
NL 162
NS 2
ND 8
Next None
Up None
Origin None
IO-Charac 2I 6F
             ---------- Description of the links ----------
1 CALO ADC channel bank
                    LQ(IEVTH-1) - address of the first CALO bank (if any)
2 MWPC MWPC bank
                    LQ(IEVTH-2) - address of the MWPC bank
             ---------- Description of the Reference links ----------
1-160 CALO Addresses of CALO banks for ADC channels 1-160
                    LQ(IEVTH-2-IADC) - address of the bank for channel IADC
                    if adrress is zero - no energy, deposited in this channel
             ---------- Description of the data words ----------
1 NEVENT Event number
2 ITRIG Trigger flag
                    (=0, if only one hit in every MWPC plane)
3 ENERGY Visible energy, deposited in the prototype [GeV]
4 EOUT Visible energy, deposited in the un-equipped part [GeV]
5 EL_XP Leakage energy to the positive X direction [GeV]
6 EL_XN Leakage energy to the negative X direction [GeV]
7 EL_YD Leakage energy through the bottom [GeV]
8 EL_ZB Leakage energy through the back [GeV]

CALO ADC channel bank

---------------------------------------------- entered file at 1-Aug-97 14:23
Bank IDH CALO ADC channel bank
Author Andrei Kiryunin
ND 3+3*NCHITS
Next CALO
Up EVTH
Origin EVTH
IO-Charac 1I 1F 1I / 1I 2F
             ---------- Description of the data words ----------
1 IADC ADC channel number
2 EADC Visible energy, deposited in the channel
3 NCHITS Number of hits
                    Information about hits:
--REP level=1 (loop over hits: 1 - NCHITS)
    1 NGAP LAr gap number (1-8) with the current hit
    2 THIT Time of flight of the hit [ns]
    3 EHIT Visible energy of the hit [GeV]
--REP level=1 -- End --

MWPC MWPC bank

---------------------------------------------- entered file at 1-Aug-97 14:23
Bank IDH MWPC MWPC bank
Author Andrei Kiryunin
ND 10+NMHITS
Next None
Up EVTH
Origin EVTH
IO-Charac 10I -F
             ---------- Description of the data words ----------
1 NX_1 Number of hits in the X-plane of MWPC 1
2 NX_2 Number of hits in the X-plane of MWPC 2
3 NX_3 Number of hits in the X-plane of MWPC 3
4 NX_4 Number of hits in the X-plane of MWPC 4
5 NX_5 Number of hits in the X-plane of MWPC 5
6 NY_1 Number of hits in the Y-plane of MWPC 1
7 NY_2 Number of hits in the Y-plane of MWPC 2
8 NY_3 Number of hits in the Y-plane of MWPC 3
9 NY_4 Number of hits in the Y-plane of MWPC 4
10 NY_5 Number of hits in the Y-plane of MWPC 5
                    NMHITS =
                    = NX_1 + NX_2 + NX_3 + NX_4 + NX_5 +
                    + NY_1 + NY_2 + NY_3 + NY_4 + NY_5
                    Information about hits:
--REP level=1 (loop over planes: X and Y)
  --REP level=2 (loop over chambers: 1 - 5)
    --REP level=3 (loop over N hits in the plane, if N>0)
            1 COOR Coordinate of a wire with the hit [cm]
    --REP level=3 -- End --
  --REP level=2 -- End --
--REP level=1 -- End --

Index CALO : : : : : : : : : : : : : : : : : 4 EVTH : : : : : : : : : : : : : : : : : 3 MWPC : : : : : : : : : : : : : : : : 5 RUNH : : : : : : : : : : : : : : : : : 2