Status of MC Simulations for the HEC Module 0

A. Kiryunin 18-March-1999

ffl Simulated data in CWNs

ffl Horizontal scan with pions

Simulated Data in Column-Wise Ntuples

ffl FZ banks ) Ntuples:

similar format as for real data (produced with HEC- ADC 3.6)

ffl MC information:

– pure MC signal in ADC channels – spoiled MC signal (disconnected sub-gaps, dead channels, absent calibration) – spoiled MC signal with noise – leakage energy

ffl Electronic noise (provided by A. Minaenko):

– ordinary noise – noise as after digital filtering

ffl Rewritten: pion and electron energy scans, muon

runs (for April and for August)

ffl http://wwwatlas.mppmu.mpg.de/HEC/tb3cwn.html

– access to ntuples – format description – list of hardware problems, taken into account

Horizontal Scan with Pions

ffl Scan with 120 GeV pions at YT ABLE=5.3 cm ffl Simulation package HEC-BEAM 3.0

(A. Kiryunin and D. Salihagić)

ffl Shower models: G-CALOR, G-FLULKA, GHEISHA ffl Reconstruction volume:

– whole module

– 109 channel tower (module without left ’-sector)

4

5

6

ffl Further simulations: are there requests? ffl Information about simulated data at MPI:

http://wwwatlas.mppmu.mpg.de/HEC/tb3.html