% --------------------------------------------------------------------
% ALMY Workshop 98 Vortrag
% Author: H. Kroha
% --------------------------------------------------------------------
%
%
%FORMAT latex % use LATEXE format
\documentstyle[dina4,epsfig,colordvi]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -10mm
\evensidemargin -10mm
\topmargin -10mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 230mm
\textwidth 180mm

\parindent0.0em

\font\tenrm=cmr10

%\pagestyle{empty}

%\psdraft

\begin{document}
%
\MyLogo{H.~Kroha, MPI Munich\hspace{6.7cm}
ALMY Workshop, MPI Munich, 6-8 April 1998}
%
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page0
%

\noindent
\begin{center}
\begin{LARGE}
\Blue{\bf Laser-Alignment System with}
\Blue{\bf Transparent Silicon Strip Sensors}
\end{LARGE}
\vspace{5mm}

\noindent
{\bf V.~Bartheld, B.~Dulny, J.~Fent, \underline{H.~Kroha}, S.~Schael}
\vspace{2mm}

\noindent
{\bf Max-Planck-Institut f\"ur Physik, Munich}
\end{center}
\vspace{35mm}

\begin{large}
\noindent
\Red{\bf High-precision optical \underline{multi-point} alignment systems.}
\hfill\break

\noindent
\Red{\bf MPA-ALMY silicon strip position sensors.}
\end{large}

\vfill\eject
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page5
%
\begin{center}
\begin{table}[t]
\noindent
\Red{Properties of Silicon Strip Photo Diodes}
\vskip 1cm

\begin{tabular}{|p{6cm}|c|c|}
%
\hline        
Sensor type & c-Si & a-Si \\ 
\hline
Active area & $20\times 20$~mm${}^2$ & $20\times 20$~mm${}^2$ \\
%
$\#$~Strips & 67 & $64\times 64$ \\
%
Strip pitch & $300~\mu$m & $312~\mu$m \\
%
Strip width & $280~\mu$m & $300~\mu$m \\
%
Si thickness & $50-300~\mu$m & $0.5-1~\mu$m \\
%
Sensitive depth & $\sim 20~\mu$m & $\sim 1~\mu$m \\
%
\hline
Band gap & $1.1~\mu$m & $0.82~\mu$m \\
%
\hline   
Transmittance & $71\%$    & $80~\%$  \\
              & (1064~nm) & (690~nm) \\
              & $80\%$    & $90\%$   \\
              & (1083~nm) & (790~nm) \\
%
\hline   
Pos.~resolution & & \\
(uncorrected over   & $<15~\mu$m & $<5~\mu$m \\
the whole surface) & $\mapsto 1~\mu$m & $\mapsto 1~\mu$m \\
\hline   
%
Hall mobility & & \\ 
%
\hspace{2mm}$\mu_p^H$~[cm${}^2$/Vs] &
310 & $10^{-4}$ \\
%
\hspace{2mm}$\mu_n^H$~[cm${}^2$/Vs] &
1650 & $10^{-2}-10^{-3}$ \\
%
\hline   
Lorentz shift\hfill\break
\hspace{3mm}(for B=4~T)
& $<1~\mu$m & $\ll 1~\mu$m \\
%
\hline
%                       
\end{tabular}
\end{table}
%
\end{center}

\eject
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page13

\begin{center}
\Blue{\framebox[6.7cm]{\Large\bf Applications}}
\vskip 2cm

{\bf
\begin{itemize}
\item
 ATLAS Muon Spectrometer

\item
 ATLAS Inner Tracker

\item
 CMS Muon Spectrometer

\item
 CMS Inner Tracker

\item
 HERA-B Silicon Vertex Detector

\item
 HERA-B Tracking Detector

\item
 ZEUS Silicon Vertex Detector

\item
 AMS Silicon telescope

\item
 NOMAD calorimeter

\item
 LHC Magnets, Accelerators, ...
\end{itemize}
}

\end{center}
\eject
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
