%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{sidewaysfigure}
%\begin{table}[p]
\renewcommand{\arraystretch}{1.10}

\begin{center}
\noindent
{\bf Table~5:} Quality control tests during chamber assembly.
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction if failed} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline

& & & &\\
\multicolumn{5}{l}{\bf Environment} \\ [1mm]

Room temperature       & $20\pm 1~\circ$C & adjust & local & before glueing \\
& & & &\\

Relative humidity      & $50\pm 10~\%$     & adjust & local & before glueing \\
& & & &\\

Atmospheric pressure   &                   &        & local & monitoring     \\
({\bf optional}) & & & &\\
& & & &\\

Temperature of outer cross plates & $20\pm 0.5^\circ$C & adjust & local & uniform, before glueing \\
& & & &\\

Temperature of end combs & $20\pm 0.5^\circ$C & adjust & local & uniform, before glueing \\
& & & &\\

Temperature difference & $<0.2^\circ$C & adjust & local & during glueing \\
outer cross plates--end combs       & & & &\\
\hline

& & & &\\
\multicolumn{5}{l}{\bf Spacer assembly} \\ [1mm]

Glue gaps between tube layer & $200-1000~\mu$m  & adjust & local & both orientations of cross plates \\
on combs and cross plates    &                  &        &       & around $z$-axis                  \\
& & & &\\
\hline

& & & &\\
\multicolumn{5}{l}{\bf On-chamber gas system} \\ [1mm]

Leak rate  & less than $10^{-8}$~bar~l/s  & repair & local & of preassembled gas manifolds \\
& & & &\\

Flow rate/tube  & to be specified  & repair & & for preassembled gas manifolds \\
& & & &\\
\hline\hline

\end{tabular}
\end{center}

%\end{table}
\end{sidewaysfigure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
