%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{sidewaysfigure}
%\begin{table}[p]
\renewcommand{\arraystretch}{1.10}

\begin{center}
\noindent
{\bf Table~7:} Quality control tests of all assembled chambers at the production sites
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction if failed} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline


& & & &\\
\multicolumn{5}{l}{\bf Mechanical Tests} \\ [1mm]

Sag of chamber &  & store data & central & $y$ readings of  \\
on kinematical supports & & & & in-plane monitors \\
before sag compensation   & & & &  \\
& & & &\\

Sag of chamber            & within $\pm 20~\mu$m  & adjust sag compensation  & central & $y$ readings of  \\
on kinematical supports   & of nominal wire sag   & until within tolerance,  & & in-plane monitors \\
after sag compensation    &                       & store data               & &  \\
& & & &\\

Deformation of cross plates  & $<20~\mu$m  & store data & central & with temporary cross \\
on kinematical supports      & & &                                & plate sag monitors \\
({\bf recommended for BM, BO}) & & & & and FEA model \\
& & & &\\

Rel.\ angular alignment of & see Table~6   & store data  & local & includes accuracy of reconstruction  \\
alignment  platforms    &               &             &         & of thermal and gravitational         \\
on kinematical supports &               &             &         & deformations with in-plane system    \\
after sag compensation  & & & &\\
& & & &\\

\hline\hline

\end{tabular}
\end{center}
\hfill

%\end{table}
\end{sidewaysfigure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
