%----------------------------------------------------------------------
\documentstyle[twoside,11pt,rep11n,epsfig,rotating,fancyheadings,here]%
{report}
%----------------------------------------------------------------------
%             page style 
%             ----------
\def\figurename{{\bf Fig.}}
\def\tablename{{\bf Table}}
%\nofiles
%\psdraft
%
%
%  position of the text on the page
\oddsidemargin=-6mm
\evensidemargin=-6mm
\topmargin=-10mm
\headheight=0.5cm
\headsep=0.5cm
\textheight=250mm
\textwidth=170mm
\topskip=1.1cm
%\footskip=2.0cm
%\footheight=0.8cm
\jot=12pt
\raggedbottom
%\parskip0ex plus0.1ex
\parskip1mm
\parindent1.5em
%
% create my own head/foot layout using the "fancyheading" style file
%
\pagestyle{empty}

%---------------------------------------------------------------------
\begin{document}
%
%--for floats (i.e. figures or tables)
\renewcommand{\topfraction}{0.8}
\renewcommand{\bottomfraction}{0.8}
\renewcommand{\thefootnote}{\fnsymbol{footnote}}
%

\fboxrule=0.5mm
\fboxsep=3mm
\parindent=0pt

%------------------------------------------       
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{sidewaysfigure}
%\begin{table}[p]
\renewcommand{\arraystretch}{0.95}

\begin{center}
\noindent
{\bf Table~8:} Quality control tests of all assembled chambers at the production sites (cont.)
\vspace{2mm}

\begin{tabular}{lllcl}

\hline\hline
& & & &\\
{\bf Test} & {\bf Acceptance criteria} & {\bf Reaction if failed} & {\bf Data base} & {\bf Comment} \\ [1mm]
\hline

& & & &\\
\multicolumn{5}{l}{\bf Operation Tests} \\ [1mm]

Gas pressure test      & test done,        & repair gas manifold,   & central  &   \\
at 3 bar overpressure  & no obvious leaks  & repair/disconnect      &          &                   \\
                       &                   & faulty tubes, store ID &          &                   \\
& & & &\\

Gas leak rate         & less than $2\times 10^{-8}$~bar~l/s  & repair gas manifold, & central & after pressure  \\
at 2 bar overpressure & per tube                             & repair/disconnect    &         & test       \\
                      &                                      & faulty tubes, store ID &       &        \\
& & & &\\

HV stability:   & less than 2~nA/m~$+5$~nA & replace electronics  & central & with installed electronics boards,  \\
leakage current & per channel            & boards; identify,    &         & baseline gas at 3 bar \\
                &                        & sputter/disconnect   &         & and nominal and $8\times$ nominal   \\
                &                        & faulty drift tubes,  &         & gas gain                            \\
                &                        & store ID             & &\\
& & & &\\

HV stability:     & within $\pm 3\sigma$     & identify noisy       & local   & with installed electronics boards,  \\
cosmic count rate & of nominal value         & channels,            &         & baseline gas at 3 bar \\
({\bf optional})  &                          & store ID             &         & and nominal gas gain  \\
& & & &\\

Operation in    & evaluation of performance: & make chamber     & local   & with test electronics,  \\
cosmic ray test & noise level, efficiency,   & operational,     &         & baseline gas at 3 bar   \\
stand           & random rate, max.\ drift time,  & store ID of &         & and nominal gas gain    \\
                & resolution vs.\ $x$, uniformity, & faulty tubes & & \\
                & local wire displacement,   & & &\\
                & stable performance of all  & & &\\
                & channels over 1--2 weeks   & & &\\
& & & &\\

Wire location   & no systematic deviations   & store wire location         & central & track reconstruction \\
measurement     & from expected wire grid    & data incl.\ meas.\ errors,  &         & in cosmic ray tower  \\
with cosmic rays&                            & adjust assembly tooling     &         &  \\
({\bf optional}) &                           & in case of deviations       & &\\
& & & &\\
\hline\hline

\end{tabular}
\end{center}
\hfill

%\end{table}
\end{sidewaysfigure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
