% --------------------------------------------------------------------
% IEEE 2000 Talk
% Author: H. Kroha
% --------------------------------------------------------------------
%FORMAT latex % use LATEXE format
\documentstyle[epsfig,rotating,colordvi,fancyheadings]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -17mm
\evensidemargin -17mm
\topmargin -30mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 265mm
\textwidth 190mm

\font\tenrm=cmr10

%\psdraft

\begin{document}

\pagestyle{fancyplain}
 \headrulewidth 0pt
 \plainheadrulewidth 0pt
 \footrulewidth 2pt
 \plainfootrulewidth 2pt
\rhead[\fancyplain{}{}]{\fancyplain{}{}}
\lhead[\fancyplain{}{}]{\fancyplain{}{}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\tiny IEEE NSS Symposium, 19/10/2000}%
{\tiny IEEE NSS Symposium, 19/10/2000}}
\cfoot{}
\lfoot[\fancyplain{}{}]%
{\fancyplain{\tiny H.~Kroha, MPI f\"ur Physik, Munich}%
{\tiny H.~Kroha, MPI f\"ur Physik, Munich}}

\fboxrule=0.8mm
\fboxsep=3mm
\parindent=0.0em

%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{figure}

\begin{center}
\Blue{\fbox{\large\bf BOS~1998 Prototype Chamber}}
\end{center}
\vspace{4mm}

{\large\bf Residuals of wire grid fit to X-ray measurements:}
\vspace{-11mm}

\begin{tabular}{ll}
\begin{minipage}{0.60\textwidth}

\hspace{-19mm}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/atlas/fortran/mun98_5_8p.eps,
width=1.14\textwidth}}
\end{minipage} &
\begin{minipage}{0.50\textwidth}

\hspace{-18mm}
{\large\bf Chamber ends:}
\vspace{3mm}

\hspace{-18mm}
\Red{\fbox{\parbox{0.81\textwidth}{
\begin{large}
{\bf Wire pos.\ accuracy}\hfill \\
{\boldmath $<18~\mu$}{\bf m (rms)}\hfill
\end{large}}}}
\end{minipage} \\ [-14mm]

\begin{minipage}{0.60\textwidth}

\hspace{-19mm}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/atlas/fortran/mun98_5_r2_10_4pp_layer_sc.eps,
width=1.14\textwidth}}
\end{minipage} &
\hspace{-12mm}
\begin{minipage}{0.50\textwidth}
{\bf Aluminum tube walls\hfill\break
(diameter} {\boldmath $\pm 15~\mu$}{\bf m)\hfill\break
used for drift tube\hfill\break
positioning during\hfill\break
assembly\hfill\break
(TDR method)}\hfill
\end{minipage} \\
\end{tabular}

\vspace{-200mm}

\end{figure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{figure}

\begin{center}
\Blue{\fbox{\large\bf BOS~2000 MDT Chamber}}
\end{center}
\vspace{4mm}

{\large\bf Residuals of wire grid fit to X-ray measurements:}
\vspace{-11mm}

\begin{tabular}{ll}
\begin{minipage}{0.60\textwidth}

\hspace{-19mm}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/atlas/fortran/bos_2000_08_p2_r0_25_8p.eps,
width=1.14\linewidth}}
\end{minipage} &
\begin{minipage}{0.50\textwidth}

\hspace{-18mm}
{\large\bf Chamber ends:}
\vspace{3mm}

\hspace{-18mm}
\Red{\fbox{\parbox{0.81\textwidth}{
\begin{large}
{\bf Wire pos.\ accuracy}\hfill \\
{\boldmath $<14~\mu$}{\bf m (rms)}\hfill
\end{large}}}}
\end{minipage} \\ [-14mm]

\begin{minipage}{0.60\textwidth}

\hspace{-19mm}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/atlas/fortran/bos_2000_08_p2_r0_25_6p_layer_sc.eps,
width=1.14\linewidth}}
\end{minipage} &
\hspace{-12mm}
\begin{minipage}{0.50\textwidth}
{\bf Precise endplugs\hfill\break
used for drift tube\hfill\break
positioning during\hfill\break
assembly.}\hfill
\end{minipage} \\
\end{tabular}

\vspace{-200mm}

\end{figure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{figure}

\begin{center}
\Blue{\fbox{\large\bf BOS~2000 MDT Chamber}}
\end{center}
\vspace{4mm}

{\large\bf Residuals of wire grid fit to X-ray measurements:}
\vspace{-11mm}

\begin{tabular}{ll}
\begin{minipage}{0.60\textwidth}

\hspace{-19mm}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/atlas/fortran/bos_2000_08_p3_r0_27_8p.eps,
width=1.14\linewidth}}
\end{minipage} &
\begin{minipage}{0.50\textwidth}

\hspace{-18mm}
{\large\bf Center of chamber:}
\vspace{3mm}

\hspace{-18mm}
\Red{\fbox{\parbox{0.81\textwidth}{
\begin{large}
{\bf Wire pos.\ accuracy}\hfill \\
{\boldmath $<10~\mu$}{\bf m (rms)}\hfill
\end{large}}}}
\end{minipage} \\ [-14mm]

\begin{minipage}{0.60\textwidth}

\hspace{-19mm}
\mbox{\epsfig{figure=/home/iwsatlas1/kroha/tex/atlas/fortran/bos_2000_08_p3_r0_27_8p_layer_sc.eps,
width=1.14\linewidth}}
\end{minipage} &
\hspace{-12mm}
\begin{minipage}{0.50\textwidth}
{\bf Variations in\hfill\break
wire sag negligible,}\hfill\break
{\bf only} {\boldmath $4~\mu$}{\bf m (rms).}\hfill
\end{minipage} \\
\end{tabular}

\vspace{-200mm}

\end{figure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
