% --------------------------------------------------------------------
% IEEE 2000 Talk
% Author: H. Kroha
% --------------------------------------------------------------------
%FORMAT latex % use LATEXE format
\documentstyle[epsfig,rotating,colordvi,fancyheadings]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -17mm
\evensidemargin -17mm
\topmargin -31mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 266mm
\textwidth 190mm

\font\tenrm=cmr10

%\psdraft

\begin{document}

\pagestyle{fancyplain}
 \headrulewidth 0pt
 \plainheadrulewidth 0pt
 \footrulewidth 2pt
 \plainfootrulewidth 2pt
\rhead[\fancyplain{}{}]{\fancyplain{}{}}
\lhead[\fancyplain{}{}]{\fancyplain{}{}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\tiny IEEE NSS Symposium, 19/10/2000}%
{\tiny IEEE NSS Symposium, 19/10/2000}}
\cfoot{}
\lfoot[\fancyplain{}{}]%
{\fancyplain{\tiny H.~Kroha, MPI f\"ur Physik, Munich}%
{\tiny H.~Kroha, MPI f\"ur Physik, Munich}}

\fboxrule=0.8mm
\fboxsep=3.5mm
\parindent=0.0em
\arraycolsep=0.0em
\baselineskip=15mm
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\begin{figure}

\begin{center}
\Blue{\fbox{\large\bf Assembly Jigging Precision}}
\end{center}
\vspace{6mm}

{\bf All components fabricated in industry, measured at MPI}
\vspace{4mm}

\begin{large}
\Blue{\bf Combs for tube positioning:}
\end{large}
\vspace{4mm}

Tube $z$ position: \Red{{\boldmath $\hphantom{30036n}\pm 4~\mu$}{\bf m} (rms)}

Tube $y$ position: \Red{{\boldmath $\hphantom{30036n}\pm 3~\mu$}{\bf m} (rms)}

$z$-pitch ($20^\circ$C): \Red{{\boldmath $30036\pm 0.5~\mu$}{\bf m} (rms)}

\vspace{6mm}

\begin{large}
\Blue{\bf Sphere towers tube layer positioning:}
\end{large}
\vspace{3mm}

\begin{tabular}{ll}
\hspace{-6mm}
\begin{minipage}{0.6\textwidth}

Layer $z$ position: \Red{{\boldmath $\hphantom{3169}\pm 3~\mu$}{\bf m} (abs.)}

Layer $y$ position: \Red{{\boldmath $\hphantom{3169}\pm 5~\mu$}{\bf m} (abs.)}

$y$-pitch: \hfill\Red{{\boldmath $26039\pm 0.5~\mu$}{\bf m} (rms)}

Spacer height: \Red{{\boldmath $346942\pm 5~\mu$}{\bf m} (rms)}

\vspace{5mm}
\mbox{\epsfig{figure=/.at/WWW/ftp/outgoing/mdt/Module0/m-machine-03.eps,height=75mm}}

\end{minipage} &
\begin{minipage}{0.4\textwidth}
\hspace{-10mm}
\mbox{\epsfig{figure=/.at/mdt_data/kroha/eps/tower-01.eps,width=1.00\textwidth}}

\vbox to 20mm{\vfill}
\end{minipage} \\
\end{tabular}

\vspace{-18mm}

\begin{center}
\mbox{\epsfig{figure=jig06.eps,width=0.84\textwidth}}
\end{center}

\vspace{-200mm}

\end{figure}

\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
