% --------------------------------------------------------------------
% Aachen 99 Vortrag
% Author: H. Kroha
% --------------------------------------------------------------------
%FORMAT latex % use LATEXE format
\documentstyle[epsfig,rotating,colordvi,fancyheadings]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -17mm
\evensidemargin -17mm
\topmargin -28mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 265mm
\textwidth 190mm

\font\tenrm=cmr10

%\psdraft

\begin{document}

\pagestyle{fancyplain}
 \headrulewidth 0pt
 \plainheadrulewidth 0pt
 \footrulewidth 1pt
 \plainfootrulewidth 1pt
\rhead[\fancyplain{}{}]{\fancyplain{}{}}
\lhead[\fancyplain{}{}]{\fancyplain{}{}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\tiny IEEE NSS Symposium, 19/10/2000}%
{\tiny IEEE NSS Symposium, 19/10/2000}}
\cfoot{}
\lfoot[\fancyplain{}{}]%
{\fancyplain{\tiny H.~Kroha, MPI f\"ur Physik, Munich}%
{\tiny H.~Kroha, MPI f\"ur Physik, Munich}}

\fboxrule=0.8mm
\fboxsep=3mm
\parindent=0.0em
\arrayrulewidth=0.8mm
\tabcolsep=2mm
\renewcommand{\arraystretch}{1.15}
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page14
%
\begin{figure}

\begin{center}
\Blue{\fbox{\Large\bf Prototype Test Beam Results}}
\end{center}
\vspace{6mm}

\begin{itemize}

\item 
\begin{large}
{\bf Operation of the prototype chamber with}\hfill

\Red{{\bf Ar:CO}{\boldmath ${}_2$} {\bf (93:7) gas mixture at 3~bar.}}\hfill\break
\end{large}
\begin{normalsize}
{\bf Gas chosen to prevent drift tube aging up to} {\boldmath $0.6$}~{\bf C/cm.}
\end{normalsize}

\begin{large}
\item {\bf Determination of}\hfill\break
\Red{\bf r-t-relation and drift tube resolution}
\end{large}

\begin{normalsize}
{\bf using the silicon strip detector beam telescope for}\hfill\break
{\bf precise track position meas.}{\boldmath $(\sigma = 11~\mu$}{\bf m):}
\end{normalsize}

\end{itemize}
\vspace{1mm}

\begin{tabular}{ll}
\hspace{-15mm}
\begin{minipage}{0.5\textwidth}
\vspace{-14mm}
\mbox{\epsfig{figure=/.at/WWW/ftp/outgoing/mdt/BOS-3800/bos98_tb_rtrel99_2.eps,
width=1.12\textwidth}} 
\end{minipage} &
%\hspace{-15mm}
\begin{minipage}{0.5\textwidth}
\mbox{\epsfig{figure=/.at/WWW/ftp/outgoing/mdt/BOS-3800/bos98_tb_resol99.eps,
width=1.12\textwidth}} 
\end{minipage} \\
\end{tabular}
\vspace{3mm}

\begin{large}
\Blue{{\boldmath $\Longrightarrow$}{\bf Average drift tube position resolution}}\hfill\break
{\boldmath $\hphantom{\Longrightarrow}$}\Blue{\bf as expected:}
\hspace{10mm}\Red{{\boldmath $70~\mu$}{\bf m (rms).}}
\end{large}
\vspace{7mm}

\begin{center}
{\boldmath $80~\mu$}{\bf m (rms) for Ar:N}{\boldmath ${}_2:$}{\bf CH}{\boldmath ${}_4$}
{\bf (91:4:5) at 3~bar}
\end{center}

\vspace{-200mm}

\end{figure}

\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
