% --------------------------------------------------------------------
% Aachen 99 Vortrag
% Author: H. Kroha
% --------------------------------------------------------------------
%FORMAT latex % use LATEXE format
\documentstyle[epsfig,rotating,colordvi,fancyheadings]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -17mm
\evensidemargin -17mm
\topmargin -25mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 260mm
\textwidth 190mm

\font\tenrm=cmr10

%\psdraft

\begin{document}

\pagestyle{fancyplain}
 \headrulewidth 0pt
 \plainheadrulewidth 0pt
 \footrulewidth 1pt
 \plainfootrulewidth 1pt
\rhead[\fancyplain{}{}]{\fancyplain{}{}}
\lhead[\fancyplain{}{}]{\fancyplain{}{}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\tiny IEEE NSS Symposium, 19/10/2000}%
{\tiny IEEE NSS Symposium, 19/10/2000}}
\cfoot{}
\lfoot[\fancyplain{}{}]%
{\fancyplain{\tiny H.~Kroha, MPI f\"ur Physik, Munich}%
{\tiny H.~Kroha, MPI f\"ur Physik, Munich}}

\fboxrule=0.8mm
\fboxsep=3mm
\parindent=0.0em
\arrayrulewidth=0.8mm
\tabcolsep=2mm
\renewcommand{\arraystretch}{1.15}
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page14
%
\begin{figure}

\begin{center}
\Blue{\fbox{\Large\bf Conclusions}}
\end{center}
\vspace{10mm}

\begin{itemize}

\item \Red{\bf The full-scale prototype of one of the largest MDT precision drift chambers
for the ATLAS muon spectrometer has been constructed in 1998 with methods
for large-scale production.}

{\bf Demonstrated that the required wire positioning accuracy of} 
\Red{{\boldmath $<20~\mu$}{\bf m (rms)}} {\bf can be achieved.}

\item \Red{\bf The test beam results show the required performance for a large
chamber with 432 drift tubes.}

{\bf The use of Ar:CO}{\boldmath ${}_2$} {\bf with only} {\boldmath $7\%$ {\bf CO}{\boldmath ${}_2$}
as drift gas requires great care in the fabrication and operation of the large number of drift tubes.}

\item \Red{\bf MDT chamber production for ATLAS has started.}

{\bf The first large production chamber has a wire}\hfill\break
{\bf positioning accuracy of} \Red{{\boldmath $14~\mu$}{\bf m (rms).}}\hfill

\item \Blue{Demonstration of the high-precision optical alignment monitoring
systems for the ATLAS muon spectrometer is in progress.}

\end{itemize}

\end{figure}

\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
