% --------------------------------------------------------------------
% Aachen 99 Vortrag
% Author: H. Kroha
% --------------------------------------------------------------------
%FORMAT latex % use LATEXE format
\documentstyle[epsfig,rotating,colordvi,fancyheadings]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -20mm
\evensidemargin -20mm
\topmargin -31mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 270mm
\textwidth 195mm

\font\tenrm=cmr10

%\psdraft

\begin{document}

\pagestyle{fancyplain}
 \headrulewidth 0pt
 \plainheadrulewidth 0pt
 \footrulewidth 1pt
 \plainfootrulewidth 1pt
\rhead[\fancyplain{}{}]{\fancyplain{}{}}
\lhead[\fancyplain{}{}]{\fancyplain{}{}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\tiny IEEE NSS Symposium, 19/10/2000}%
{\tiny IEEE NSS Symposium, 19/10/2000}}
\cfoot{}
\lfoot[\fancyplain{}{}]%
{\fancyplain{\tiny H.~Kroha, MPI f\"ur Physik, Munich}%
{\tiny H.~Kroha, MPI f\"ur Physik, Munich}}

\fboxrule=0.8mm
\fboxsep=3mm
\parindent=0.0em
\arrayrulewidth=0.8mm
\tabcolsep=2mm
\renewcommand{\arraystretch}{1.15}
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page4
%
\begin{figure}
\begin{center}
\begin{Large}
\Blue{\fbox{\bf Monitored Drift Tube Chambers}}
\end{Large}
\end{center}

\vspace{4mm}
\begin{center}
\mbox{\epsfig{figure=/.at/mdt_data/kroha/bos_photo_11.eps,angle=-90,width=0.92\textwidth}}
\end{center}

\vspace{-2mm}
\begin{itemize}

\item \Red{{\bf Very high mechanical precision:} {\boldmath $<20~\mu$}{\bf m (rms).}}
\vspace{-4mm}

\item \Red{{\bf High reliability, no aging over} {\boldmath $>10$} {\bf years}\hfill\break
{\bf under LHC irradiation conditions.}}
\vspace{-4mm}

\item \Blue{{\bf 1200 MDT chambers with in total 400000 drift tubes}\hfill\break
{\bf covering an area of 5500~m}{\boldmath ${}^2.$}}
\vspace{-4mm}

\item \Blue{\bf Construction of 1 chamber every 2 weeks\hfill\break
at 13 production sites over 4 years.}
\vspace{-2mm}

{\bf Munich: 88 chambers with 432 drift tubes of 3.8~m length.}
\vspace{-4mm}

\item \Red{\bf High precision optical alignment monitoring system:}\hfill\break
{\bf muon sagitta corrections to}
\Red{{\boldmath $<30~\mu$}{\bf m (rms).}}

\end{itemize}

\vspace{-200mm}

\end{figure}
\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
