% --------------------------------------------------------------------
% Aachen 99 Vortrag
% Author: H. Kroha
% --------------------------------------------------------------------
%FORMAT latex % use LATEXE format
\documentstyle[epsfig,rotating,colordvi,fancyheadings]{foils}
% ---------------------------------------------------------------------
\oddsidemargin  -14mm
\evensidemargin -14mm
\topmargin -40mm
%\headheight 12pt
%\headsep 25pt
%\footheight 12pt
%\footskip 75pt
\textheight 275mm
\textwidth 185mm

\font\tenrm=cmr10

%\psdraft
\setcounter{page}{5}

\begin{document}

\pagestyle{fancyplain}
 \headrulewidth 0pt
 \plainheadrulewidth 0pt
 \footrulewidth 1pt
 \plainfootrulewidth 1pt
\rhead[\fancyplain{}{}]{\fancyplain{}{}}
\lhead[\fancyplain{}{}]{\fancyplain{}{}}
\rfoot[\fancyplain{}{}]%
{\fancyplain{\tiny IEEE NSS Symposium, 7 November, 2001}%
{\tiny IEEE NSS Symposium, 7 November, 2001}}
\cfoot{\tiny\thepage}
\lfoot[\fancyplain{}{}]%
{\fancyplain{\tiny H.~Kroha, MPI f\"ur Physik, Munich}%
{\tiny H.~Kroha, MPI f\"ur Physik, Munich}}

\fboxrule=0.8mm
\fboxsep=3mm
\parindent=0.0em
\arrayrulewidth=0.8mm
\tabcolsep=2mm
\renewcommand{\arraystretch}{1.15}
%%%%%%%%%%%%%%%%%%%%%%%%%%%
% Page17
%
\begin{figure}

\begin{center}
\hspace{-15mm}\mbox{\epsfig{figure=/home/pcatlas17/kroha/eps/ep99_3d_color.eps,
width=1.1\textwidth}}
\vspace{-25mm}

\mbox{\hspace{-17mm}\epsfig{figure=/.at/wwwatlas/ftp/outgoing/mdt/tubes/Wiring_Line/mdt_tube_2.eps,
width=1.13\textwidth}}
\end{center}
\vspace{-6mm}

\textBlue
\begin{itemize}
\addtolength{\itemindent}{-2.5mm}

\item[\Red{$\bullet$}]
{\bf Precision aluminum tubes:}\hfill\break
\Black{\small {\boldmath $29970\pm 15~\mu$}{\bf m outer diameter,}
{\boldmath $400\pm 30~\mu$}{\bf m wall thickness.}}
\vspace{-6mm}

\item[\Red{$\bullet$}]
{\normalsize\bf
Precise mechanical wire positioning with respect to precisely machined 
external reference surfaces.
}
\vspace{-6mm}

\item[\Red{$\bullet$}]
{\normalsize\bf
Injection moulded plastic insulator}\hfill\break
\Black{\small\bf (Noryl: little shrinkage, minimise stresses).}
\vspace{-6mm}

\item[\Red{$\bullet$}]
{\normalsize\bf
Wire fixation by crimping in metal insert.
}
\vspace{-6mm}

\item[\Red{$\bullet$}]
{\normalsize\bf
O-ring gas seals.
}
\vspace{-6mm}

\item[\Red{$\bullet$}]
{\normalsize\bf
Ground contact to aluminum tubes by laser spot welding.
}
\vspace{-6mm}

\item[\Red{$\bullet$}]
{\normalsize\bf
All materials tested with respect to aging.
}

\end{itemize}
\textBlack

\vspace{-270mm}
\begin{center}
\Blue{\fbox{\Large\bf Drift Tube Design}}
\end{center}

\end{figure}

\clearpage
%%%%%%%%%%%%%%%%%%%%%%%%%%%
\end{document}
